Threading the Machine

**BOBBIN:**

1. Slide the bobbin cover latch to the right, and remove the bobbin cover.



2. Hold the bobbin so it spins COUNTER-CLOCKWISE!



3. Insert bobbin into the bobbin case.



4. Guide the thread with your left hand through the slot as shown. Follow the arrows to the thread cutter and cut the end of the thread.



5. Reattach the bobbin cover – insert the tab in the lower left corner and lightly press down on the right side

